

Where Unit1LED is output left bit and Unit0LED is output right bit.



